

TruVision TVD-2403/4403 TVI Dome Camera A&E Specifications



# The TVD-2403/4403 Camera shall capture and transmit video over an analog connection.

# The TVD-2403/4403 shall be as manufactured by Interlogix.

# The TVD-2403/4403 shall include, but not be limited to the following:

## The TVD-2403/4403 shall provide analog connection for the purpose of allowing users to integrate it with TVI digital video recorder or TVI digital video encoder products.

### The TVD-2403/4403 shall provide 1 channels of TVI video output.

### The TVD-2403/4403 shall provide 1 channels of 960H composite video output.

### The TVD-2403/4403 shall include a sensor of 1/3" CMOS image sensor.

## The TVD-2403/4403 shall have effective pixels (H x V) in or over 1920 × 1080.

## The TVD-2403/4403 shall support TVI output resolution (H x V) in 1920 × 1080.

## The TVD-2403/4403 shall have 2.8mm lens.

## The TVD-2403/4403 shall have IR Cut Filter.

## The TVD-2403/4403 shall conform to IP66.

## The TVD-2403/4403 shall have up to 20m IR illumination range.

## The TVD-2403/4403 shall support 120dB Wide Dynamic Range on TVI video image.

## The TVD-2403/4403 shall have On Screen Display over coax cable control function.

## The TVD-2403/4403 shall be user configured via the internal menu.

### TVD-2403/4403 shall have an integrated menu to configure the following information:

#### Scene

#### Lens

#### Exposure

#### Backlight

#### White Balance

#### Day & Night

#### NR

#### Special

#### Adjust

#### Reset

### Configurable options shall include:

#### Scene

##### Indoor

##### Outdoor

##### Indoor1

##### Low-light

#### Lens

##### Manual

#### Exposure

##### Shutter

##### AGC

##### SENS-UP

##### Brightness

##### D-WDR

##### Defog

#### Backlight

##### BLC

##### HSBLC

#### White Balance

##### ATW

##### AWC-SET

##### Indoor

##### Outdoor

##### Manual

#### Day & Night

##### Color

##### B/W

##### Ext

#### NR

##### 2D NR

##### 3D NR

#### Special

##### CAM TITLE

##### D-EFFECT

##### Motion

##### Privacy

##### Defect

##### Version

#### Adjust

##### Sharpness

##### Monitor

##### LSC

#### Reset

##### Camera reset

# The TVD-2403/4403 shall have the following additional specifications:

## Video

### Video output: 1\*1080P TVI output and 1\*960H composite dual output

### Minimum illumination: 0.01 Lux @ (F1.2, AGC ON), 0.034 Lux @ F2.2, AGC ON), 0 Lux with IR on

## Electrical

### Power supply: 12 VDC

### Current: 0.33 A

### Power consumption: 4 W

## Environmental

### Operating temperature range: -30 to +60 °C (-22 to +140 °F)

### IP66

## Physical

### Dimensions: Ø70 × 149.5 mm (Ø2. 76 × 5. 89 in.)

### Weight: 309 g (0.68 lbs.)

# The TVD-2403/4403 shall conform to these internationally recognized compliance standards:

## FCC

## CE

## UL

## WEEE

## RoHS

## REACH

Contacting Support

North America:

855-286-8889

[techsupport@interlogix.com](mailto:techsupport@interlogix.com)

Latin America:

561-998-6114

[latam@interlogix.com](mailto:latam@interlogix.com)

Web site:

[www.interlogix.com/customer-support](http://www.interlogix.com/customer-support)

EMEA:

See specific country listings at:

[www.utcfssecurityproducts.eu/support](http://www.utcfssecurityproducts.eu/support)