

TVK-800 IP Keypad A&E Specifications



# TVK-800 shall capture snapshots, and decode video over a network.

# TVK-800 shall be as manufactured by Interlogix.

# TVK-800 shall include, but not be limited to the following:

## TVK-800 shall support PoE (802.3af) power supply.

## TVK-800 shall provide a 7” TFT LCD monitor with touch panel.

## TVK-800 shall provide a 4-axis joystick.

## TVK-800 shall provide a USB port.

## TVK-800 shall be user configured via Ethernet with a personal computer running included, and a current version of the Internet Explorer web browser.

### TVK-800 shall have an integrated web client interface to configure, upgrade, and view the following information:

#### Import/export configure file

#### Configure system settings, which include network settings

#### Configure keypad settings and user settings

#### View the system information

### Access to menus shall be set by user status.

#### Admin shall grant access to all menus.

#### Manager shall grant access to create or delete other users, assign devices, see live view or play back videos.

#### Operator/Custom shall grant access to the devices that are assigned to him.

### Configurable options shall include:

#### Search

##### Recorded video of DVR and NVR

#### Archive

##### Recorded video

##### Snapshot

#### Users

##### Add User

##### Edit User

##### Assign device

#### Alarms

##### System Notification

###### Network Disconnected

###### IP Address conflicted

#### IP Settings

##### Basic Settings

##### FTP

##### Interface

##### Network RJ-45

# The IP dome camera shall have the following operational features:

## Recording

### TVK-800 shall record video on USB and FTP.

### The user shall be able to play back videos smoothly at normal or fast speeds.

## Connections

### TVK-800 shall include the following connectors:

#### 1, RJ45 100M/1000M adaptive Ethernet port

#### 1, Line In, 3.5 mm connector (2.0 Vp-p, 1 kΩ)

#### 1, Audio Out, 3.5 mm connector (Linear, 600 Ω)

#### 1, RS-485

#### 1, RS-232

#### 1, USB

## Ethernet communications

### TVK-800 shall support 100/1000M Base T networks.

### TVK-800 shall support Dynamic IP Addressing (DHCP).

### TVK-800 shall support FTP.

# TVK-800 shall have the following additional specifications:

## Electrical

### Power supply: 12 VDC, PoE (IEEE 802.3af)

## Environmental

### Operating temperature range: -10 to +50 °C

## Physical

### Dimensions: 193 × 435 × 110 mm

### Weight: 2040 g

# TVK-800 shall conform to these internationally recognized compliance standards:

## FCC

## CE

## UL

## REACH

## RoHS

## HALT

## WEEE

Contacting Support

North America:

855-286-8889

techsupport@interlogix.com

Latin America:

561-998-6114

latam@interlogix.com

Web site:

[www.interlogix.com/customer-support](http://www.interlogix.com/customer-support)

EMEA:

See specific country listings at:

[www.utcfssecurityproducts.eu/support](http://www.utcfssecurityproducts.eu/support)