

TruVision TVB-2201/4201 Bullet Camera A&E Specifications



# The TVB-2201/4201 camera shall capture and transmit video over an analog connection.

# The TVB-2201/4201 shall be as manufactured by Interlogix.

# The TVB-2201/4201 shall include, but not be limited to the following:

## The TVB-2201/4201 shall provide analog connection for the purpose of allowing users to integrate it with digital video recorder or digital video encoder products.

### The TVB-2201/4201 shall provide 1 channel of analog video output.

### The TVB-2201/4201 shall include a sensor of 1/3" image sensor.

## The TVB-2201/4201 shall support up to 700 TV Line.

## The TVB-2201/4201 shall have effective pixels (H x V) in 976 × 496.

## The TVB-2201/4201 shall have 3.6 mm lens.

## The TVB-2201/4201 shall have IR Cut Filter.

## The TVB-2201/4201 shall conform to IP66.

## The TVB-2201/4201 shall have over 20m IR illumination range.

# The TVB-2201/4201 shall have the following additional specifications:

## Video

### Video output: 1 Vpp composite output (75 ohm/BNC)

### Min. Illumination: 0.1 Lux @ (F1.2, AGC ON), 0 Lux with IR

## Electrical

### Power supply: 12 VDC

### Current: 333 mA

### Power consumption: Max. 4W

## Environmental

### Operating temperature range: -40 to +60 °C (-40 to 140 °F)

### IP66

## Physical

### Dimensions: Ø70 × 149.5 mm (Ø2. 76” × 5. 89”)

### Weight: 360 g (0.79 lbs.)

# The TVB-2201/4201 shall conform to these internationally recognized compliance standards:

## FCC

## CE

## UL

## WEEE

## RoHS

## REACH

Contacting Support

North America:

855-286-8889

techsupport@interlogix.com

Latin America:

561-998-6114

latam@interlogix.com

Web site:

[www.interlogix.com/customer-support](http://www.interlogix.com/customer-support)

EMEA:

See specific country listings at:

[www.utcfssecurityproducts.eu/support](http://www.utcfssecurityproducts.eu/support)