

TruVision TVB-2401/4401 TVI Bullet Camera A&E Specifications



# The TVB-2401/4401 Camera shall capture and transmit video over an analog connection.

# The TVB-2401/4401 shall be as manufactured by Interlogix.

# The TVB-2401/4401 shall include, but not be limited to, the following:

## The TVB-2401/4401 shall provide analog connection for the purpose of allowing users to integrate it with TVI digital video recorder or TVI digital video encoder products.

### The TVB-2401/4401 shall provide 1 channel of TVI video output.

### The TVB-2401/4401 shall include a sensor of 1/3" CMOS image sensor.

## The TVB-2401/4401 shall have effective pixels (H x V) in or over 1280 × 720.

## The TVB-2401/4401 shall support TVI output (H x V) in 1280 × 720.

## The TVB-2401/4401 shall have 3.6 mm lens.

## The TVB-2401/4401 shall have IR Cut Filter.

## The TVB-2401/4401 shall conform to IP66.

## The TVB-2401/4401 shall have over 20 m IR illumination range.

# The TVB-2401/4401 shall have the following additional specifications:

## Video

### Video output: 1\*HD-TVI output

### Minimum illumination: 0.01 Lux @ (F1.2,AGC ON), 0.034 Lux @ F2.2,AGC ON), 0 Lux with IR on

## Electrical

### Power supply: 12 VDC

### Current: 300 mA

### Power consumption: 3.5 W

## Environmental

### Operating temperature range: -30 to +60 °C (-22 to +140 °F)

### IP66

## Physical

### Dimensions: Φ70 × 149.5 mm (Ø2. 76 × 5. 89 in.)

### Weight: 291 g (0.64 lbs.)

# The TVB-2401/4401 shall conform to these internationally recognized compliance standards:

## FCC

## CE

## UL

## WEEE

## RoHS

## REACH

Contacting Support

North America:

855-286-8889

[techsupport@interlogix.com](mailto:techsupport@interlogix.com)

Latin America:

561-998-6114

[latam@interlogix.com](mailto:latam@interlogix.com)

Web site:

[www.interlogix.com/customer-support](http://www.interlogix.com/customer-support)

EMEA:

See specific country listings at:

[www.utcfssecurityproducts.eu/support](http://www.utcfssecurityproducts.eu/support)