

TruVision TVP-2401/4401 (Wall Mount) and TVP-2402/4402 (Surface/Flush Mount) HD-TVI 30X PTZ Camera A&E Specifications



# The TruVision TVP-2401/4401 (Wall Mount) and TVP-2402/4402 (Surface/Flush Mount) HD-TVI 30X PTZ Dome Camera shall capture and transmit video over an analog connection.

# The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall be as manufactured by Interlogix.

# The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall include, but not be limited to the following:

## The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall provide analog connection for the purpose of allowing users to integrate it with digital video recorder or digital video encoder products.

### The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall provide 1 channel of analog video output.

### The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall include a sensor of 1/2.8’’ CMOS.

## The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall support up to 2 MPX TVI (Color) and 960H (B&W).

## The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall have Varifocal auto iris lens 4~120 mm.

## The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall have total pixels (H x V) in: NTSC: 1920 × 1080 / PAL: 1920 × 1080.

## The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall have S/N ratio: 52 dB.

## The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall have minimum illumination: 0.02 Lux @ F1.6 (Color) and 0.002 Lux @ F1.6 (B/W).

## The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall be user configured via the internal menu.

### The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall have an integrated menu to configure the following information:

#### Focus mode

#### Zoom limit

#### Zoom speed

#### Slow shutter

#### IR CUT filter

#### D/N level

#### Sharpness

#### Saturation

#### Contrast

#### Gain

#### HLC

#### BLC/WDR

#### White balance

#### AE mode

#### Iris

#### Shutter

#### Exposure compensation

#### Mirror

#### Noise reduction

#### Chroma suppress

#### Privacy Mask

#### Camera ID

#### Language

#### Camera reset

# The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall have the following operational features:

## Shutter speed: 1, 2, 4, 8, 15, 30, 50, 125, 180, 250, 500, 1000, 2000, 4000 or 10000.

## Iris: 0 to 17

## BLC/WDR: ON and OFF

## Contrast: 0 to 7

## Sharpness: 0 to 15

## Saturation: 0 to 7

## Gain: 0 to 15

## AE mode: AUTO, IRIS, SHUTTER, MANUAL

## Mirror: ON and OFF

## White Balance: AUTO/ INDOOR/ OUTDOOR/ SELFDEF/ ATW/ HAUTO

## Privacy Mask:

### Blank number: 24 areas can be configured.

### Blank status: ON and OFF

## Preset Tour:

### Number: 8 preset tours can be configured.

### Dwell time: 0-30s

### Speed: 1-40

## Shadow Tour

## Time Task

### Task Action: Task Action: preset, preset tour, shadow tour, pan scan, tilt scan, panorama, frame scan, random scan, patrol D, day mode, night mode, zero calibrate and none.

### Task Time

## Alarm

### Priority: High, Middle, Low.

### Alarm Action

## Connection

### The TruVision TVP-2401/4401 and TVP-2402/4402 PTZ Dome Camera shall include the following connectors:

#### Video Output: 1Vp-p composite video output

# The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall have the following additional specifications:

## Video

### Video output: 1 Vpp composite output (75 ohm/BNC)

## Electrical

### Power supply: 24 VAC ± 15%

## Environmental

### Operating temperature range:

Outdoor PTZ Camera: -30°C to 65°C

Indoor PTZ Camera: -10°C to 50°C

## Physical

### Dimensions:

Outdoor PTZ Camera: Ø 220 × 305 mm

Indoor PTZ Camera: Ø 183.4 × 243 mm

### Weight:

Outdoor PTZ Camera: 3.0 kg

Indoor PTZ Camera: 3.0 kg

# The TruVision TVP-2401/4401 and TVP-2402/4402 HD-TVI 30X PTZ Dome Camera shall conform to these internationally recognized compliance standards:

## UL

## FCC

## CE

## RoHS

## REACH

## WEEE

Contacting Support

North America:

855-286-8889

techsupport@interlogix.com

Latin America:

561-998-6114

latam@interlogix.com

Web site:

[www.interlogix.com/customer-support](http://www.interlogix.com/customer-support)

EMEA:

See specific country listings at:

[www.utcfssecurityproducts.eu/support](http://www.utcfssecurityproducts.eu/support)