### Power Supply KTP-24-4I-400

1. 24 VAC multiple outlet indoor power supply with four isolated and fused 24 VAC outputs, 400 VA
	1. The KTP-24-4I-400 power supply shall be as manufactured by GE Security or an approved equal.
	2. The power supply shall meet or exceed the following specifications:
		1. The design shall consist of a beige steel wall-mount housing.
			1. The housing shall have a locking door.
		2. The power supply shall provide up to four isolated 24 VAC outputs.
		3. The power supply shall provide resettable fuses for each output.
		4. PTC protected outputs shall meet Class 2, power limited, requirements.
	3. The electrical specifications for the power supply shall be as follows:
		1. Input voltage: 120 VAC
		2. Input power: 400 VA
		3. Output voltage: 24 VAC
		4. Output power: 100 VA
	4. The environmental specifications for the power supply shall be as follows:
		1. Operating temperature shall be 14 to 122 degrees Fahrenheit or -10 to 50 degrees Celsius.
		2. Relative humidity shall be up to 90 percent, noncondensing.
	5. The physical specifications for the power supply shall be as follows:
		1. Dimensions shall be 12 x 12 x 4 inches or 305 x 305 x 102 mm.
		2. Nominal weight shall be 18.5 pounds or 8.5 kg.
	6. The power supply shall conform to these internationally recognized compliance standards:
		1. UL

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IMAGES\ge_monogram_black.jpg | Mailing Address4575 Research Way, Suite 250Corvallis, OR 97333 USAwww.GESecurity.com | Americas800-469-1676 (US only)tel 541-754-9133fax 541-754-7162 | Asiatel 852-2907-8108fax 852-2142-5063Australiatel 61-3-9259-4700fax 61-3-9259-4799 | Europetel 32-2-725-11-20fax 32-2-721-86-13Latin Americatel 305-593-4301fax 305-267-4300 |
| © 2004 GE Security. As a company of innovation, GE Security reserves the right to change product information without notice. For the latest product specifications, visit GE Security online at www.GESecurity.com or contact your GE Security sales representative.  |