### MVC-15HS

1. 15-inch high resolution color monitor
   1. The 15-inch color CCTV monitor shall be as manufactured by GE Security or an approved equal. The monitor shall have a CRT screen with 15-inch diagonal viewing area and be contained in a metal cabinet.
   2. The monitor shall meet or exceed the following specifications:
      1. The monitor shall incorporate a 15-inch color CRT screen.
      2. The monitor shall have a maximum horizontal resolution of 800 television lines.
      3. The monitor shall have a dual scanning system that is NTSC and PAL compatible.
         1. The scanning frequency shall be 15.734 KHz / 60 Hz NTSC and 15.625 KHz / 50 Hz PAL.
      4. The monitor shall have built-in microprocessor digital control.
      5. The monitor shall have a metal cabinet with ergonomic handles built into the sides.
      6. The monitor shall use the following signal input:
         1. Composite video 1.0 V p-p at 75 ohms
      7. The monitor shall use the following video connections:
         1. BNC in/out
         2. Y/C (S-video) in/out
      8. The monitor shall use the following audio connections:
         1. RCA in/out
      9. The monitor shall have one audio speaker.
      10. The monitor shall have the following front control panel buttons:
          1. Power on/off
          2. OSD (menu)
          3. Brightness
          4. Contrast
          5. Enter
      11. The monitor shall have the following options for adjustment in an onscreen display menu:
          1. Color
          2. Tint
          3. Brightness
          4. Contrast
          5. Volume
   3. The electrical specifications for the monitor shall be as follows:
      1. Power input shall be 100 to 240 VAC, 50/60 Hz
      2. Power consumption shall be 95 W maximum.
   4. The environmental specifications for the monitor shall be as follows:
      1. Operating temperature shall be 14 to 122 degrees Fahrenheit or -10 to 50 degrees Celsius.
      2. Operating humidity shall be 10 to 90 percent.
   5. The physical specifications for the monitor shall be as follows:
      1. Net weight shall be 33 pounds or 15 kilograms.
      2. Dimensions shall be 14.21 (H) x 14.49 (W) x 14.80 (D) inches or 361 x 368 x 376 mm.
   6. The monitor shall conform to these internationally recognized compliance standards:
      1. FCC
      2. CE
      3. UL

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IMAGES\ge_monogram_black.jpg | Mailing Address 4575 Research Way, Suite 250 Corvallis, OR 97333 USA  www.GESecurity.com | Americas 800-469-1676 (US only) tel 541-754-9133 fax 541-754-7162 | Asia tel 852-2907-8108 fax 852-2142-5063  Australia tel 61-3-9259-4700 fax 61-3-9259-4799 | Europe tel 32-2-725-11-20 fax 32-2-721-86-13  Latin America tel 305-593-4301 fax 305-267-4300 |
| © 2004 GE Security. As a company of innovation, GE Security reserves the right to change product information without notice. For the latest product specifications, visit GE Security online at www.GESecurity.com or contact your GE Security sales representative. | | | | |