Release Notification	
Release Name:	Topaz 1.5 Patch  05	
Customer targeted:	Topaz 1.5	
QIT number:	46353603	
SDR Number(s):		
Urgency (High, Medium, Low):	Medium	
Note:	Patch 05 supersedes Patch 04	

Issue Description

Setup Alarm Point and go to Options page. Select Alarm Links to Relay # and set to 17. Relay 17 should be the Aux Relay for Reader 0. Instead of tripping the Aux Relay for Reader 0 it trips Relay 16 which is the Door Strike Relay. If you set it to Link with Relay # 18 then it trips Relay 17 and so on.

NOTE: Patch 05 supersedes Patch 04 because Patch 05 includes the legacy printer setup fix implemented in Patch 04 as follows:   

When you setup a Legacy printer in Windows and try to select it from the Topaz 1.5 software is causes the mp.exe to stop running.

When you load the drivers to create a printer from one of the legacy printers like the Eltron P310 or Fargo C11_16 and then go into Badge Design and access the Printer selection option instead of a list that lets you pick a Windows printer it brings up the old printer list. If you select the printer you loaded (doesn't seem to matter which one it is) and click OK and the badgercfg.dt file is updated it kills the mp.exe process and crashes the software. You are unable to successfully restart the software until you delete the badgerfg.dt file.

Steps To Apply Patch:

1.	Shutdown Topaz application. 

2.	On each machine with Topaz installed, use Windows Explorer to go to the Topaz directory: 

C:\Program Files\GE\Topaz\

3.	Make a backup copy of the following existing file: MP.exe
 by both renaming the file and copying the file to another folder. 

4.	Copy the zip file: Topaz 1.5 Patch 05.zip to the folder: 

C:\Temp 
on the local machine. Double click the zip file and extract all files. 
5. Copy the new file: MP.exe

From folder:	C:\Temp

Into folder:	C:\Program Files\GE\

6.	After completing the previous steps start Topaz application.